IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "C:\Users\PORKDMI\Desktop\CH Heavy\Готово\Коннекторы Оглаенд\Опорная пластина CH-100-B-O4 OC\v6\Модель\Опорная пластина CH-100-B-O4 OC _ SP21705.ifc"
Time stamp: "2025-09-05T08:26:06"
Preprocessor: "IFCConverter v1.0"
Originating system: "KOMPAS-3D 23.0.2285"
Application: "KOMPAS-3D 23.0.2285" version "23.0" identifier "KOMPAS-3D" by Organization (no name given)

People and organizations
  Person (no name given) (roles: "Разработал" ENGINEER) of Organization (no name given)
  Owner history of Person (no name given) (roles: "Разработал" ENGINEER) of Organization (no name given) | application "KOMPAS-3D 23.0.2285" version "23.0" identifier "KOMPAS-3D" by Organization (no name given) | change MODIFIED | created 1757049966 (2025-09-05T05:26:06Z) | last modified by Person (no name given) (roles: "Разработал" ENGINEER) of Organization (no name given) with "KOMPAS-3D 23.0.2285" version "23.0" identifier "KOMPAS-3D" by Organization (no name given)

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "Default project" | phase "MODIFIED"
  IFCSITE "Default project"
    IFCBUILDING "Default building"
      contains 3 elements
        3 x IFCBUILDINGELEMENTPROXY | names: "Пластина опорная S-M BP-200х200х8 CS", "Кронштейн приварной S-M WB-CH-100-4 CS", "Опорная пластина CH-100-B-O4 OC" | property sets: System, (unnamed)

Property sets
  System | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Масса = 2.47731 (IFCREAL) [KILO GRAM]
    Материал = "Сталь 09Г2С ГОСТ 19281-2014" (IFCLABEL)
    Наименование = "Пластина опорная S-M BP-200х200х8 CS" (IFCLABEL)
    Обозначение = "80954E" (IFCLABEL)
    Позиция = "1" (IFCLABEL)
  System | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Масса = 2.913282 (IFCREAL) [KILO GRAM]
    Материал = "Сталь 09Г2С ГОСТ 19281-2014" (IFCLABEL)
    Наименование = "Кронштейн приварной S-M WB-CH-100-4 CS" (IFCLABEL)
    Обозначение = "PS30233" (IFCLABEL)
    Позиция = "2" (IFCLABEL)
  System | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Масса = 0.045531 (IFCREAL) [KILO GRAM]
    Материал = "Сталь 10 ГОСТ 1050-2013" (IFCLABEL)
    Наименование = "Опорная пластина CH-100-B-O4 OC" (IFCLABEL)
    Обозначение = "SP21705" (IFCLABEL)
    Форматы листов документа = "A4, A3" (IFCLABEL)
  (unnamed) | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    __BodyColor = "#909090" (IFCLABEL)
    __BodyName = "Тело 1" (IFCLABEL)
    __ComponentColor = "#909090" (IFCLABEL)
    __ComponentName = "Пластина опорная S-M BP-200х200х8 CS" (IFCLABEL)
  (unnamed) | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    __BodyColor = "#909090" (IFCLABEL)
    __BodyName = "Тело 1" (IFCLABEL)
    __ComponentColor = "#909090" (IFCLABEL)
    __ComponentName = "Кронштейн приварной S-M WB-CH-100-4 CS" (IFCLABEL)
  (unnamed) | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    __BodyColor = "#909090" (IFCLABEL)
    __BodyName = "Тело 1" (IFCLABEL)
    __ComponentColor = "#909090" (IFCLABEL)
    __ComponentName = "Опорная пластина CH-100-B-O4 OC" (IFCLABEL)